主图+3-5张细节图

MODEL**：(C)ENTER SERIES**

标题：

LVCO EBIKE BBS01 36V 250W Mid Drive Kit

**PRODUCT**

**160N.m Torque CENTER DIRVE EASY ASSEMBLY/Efficiency**

LVCO mid-mounted motor is easy to install and is suitable for bicycles with a bottom bracket width of 68/100/120mm;The motor is small in size and has a large torque. The maximum 160N.m can provide super-strong explosive force for the vehicle;It adopts vector controller, high reliability and high efficiency drive unit, low power consumption and longer mileage.



**DETAILS**

EBIKE BBS01 36V 250W Mid Drive Kit

|  |  |
| --- | --- |
| **Size** | 25\*136\*101MM |
| **Rated Voltage** | **36V/48V** |
| **Rated power** | 250w/350w/500w |
| **Max speed** | 30km/h |
| **Torque** | 145N.m |
| **Weight** | 4kgs |
| **Sensor** | Speed sensor |
| **IP** | 65 |
| **Dispaly** | **LCD** |